Information about AppImage: https://appimage.org/

A short video about the launch of AntScope2 in Ubuntu: https://www.facebook.com/RigExpertUkraineLtd/videos/893913100945907/

To configure the RigExpert analyzers in Linux, do the following: 

sudo adduser $USER dialout

insert the file rigexpert-usb.rules to /etc/udev/rules.d



Version info:

1.0.1 - initial version

1.0.3 - Bug fix

1.0.4 - Fix logo

1.0.5 - Fix markers and more...

1.0.10 	- Layouts improved
	- Calibration bug fixed
	- ITU-region switching implemented
	- Ukrainian and Russian localization edited
	- HELIAX, LRM and M&P cables parameters added
	- Some minor bugs fixed

1.0.11 - Fix some minor bugs. Added the ability to open files created by AntScope1.

1.0.13 - Bugs fix. Added new coax cables.
	- AA-30.ZERO support
	- Belarus analyzer support
	- AA-2000 screenshots implemented
	- AA-2000 & AA-230 Stick added

1.0.14 	- analyzer detection improved
	- developer mode
   	- start measurements in tab "User defined"/"ï¿½ï¿½ï¿½ï¿½ï¿½ï¿½ï¿½ï¿½ï¿½ï¿½ï¿½' (last tab) will send EFRX command to analyzer. If analyzer supports this feature, it will send, user defined data in addition to F, R, X.
    	- start measurements with range=0 will start "One FQ" mode. (Not all analyzers support this feature correctly) 


Antscope2 1.2.1
What's new:
- NanoVNA H4 support added
- NanoVNA SAA2 support added 
- minor bugs fixed

Antscope2 1.2.2
- Minor bugs fixing

AntScope2 1.2.5
- - The notification system has been improved.
